Synergy Configuration
  Board "S1JA TB"
  R7FS1JA783A01CFM
    part_number: R7FS1JA783A01CFM
    rom_size_bytes: 262144
    ram_size_bytes: 32768
    data_flash_size_bytes: 8192
    package_style: LQFP
    package_pins: 64
    
  S1JA
    series: 1
    
  S1JA Family
    OFS0 register settings: Select fields below
         IWDT Start Mode: IWDT is Disabled
         IWDT Timeout Period: 2048 cycles
         IWDT Dedicated Clock Frequency Divisor: 128
         IWDT Window End Position:  0% (no window end position)
         IWDT Window Start Position: 100% (no window start position)
         IWDT Reset Interrupt Request Select: Reset is enabled
         IWDT Stop Control: Stop counting when in Sleep, Snooze mode, or Software Standby
         WDT Start Mode Select: Stop WDT after a reset (register-start mode)
         WDT Timeout Period: 16384 cycles
         WDT Clock Frequency Division Ratio: 128
         WDT Window End Position:  0% (no window end position)
         WDT Window Start Position: 100% (no window start position)
         WDT Reset Interrupt Request: Reset
         WDT Stop Control: Stop counting when entering Sleep mode
    OFS1 register settings: Select fields below
         Voltage Detection 0 Circuit Start: Voltage monitor 0 reset is disabled after reset
         Voltage Detection 0 Level: 1.90 V
         HOCO OScillation Disable: HOCO oscillation is disabled after reset
    MPU - Enable or disable PC Region 0: Disabled
    MPU - PC0 Start: 0x000FFFFC
    MPU - PC0 End: 0x000FFFFF
    MPU - Enable or disable PC Region 1: Disabled
    MPU - PC1 Start: 0x000FFFFC
    MPU - PC1 End: 0x000FFFFF
    MPU - Enable or disable Memory Region 0: Disabled
    MPU - Memory Region 0 Start: 0x000FFFFC
    MPU - Memory Region 0 End: 0x000FFFFF
    MPU - Enable or disable Memory Region 1: Disabled
    MPU - Memory Region 1 Start: 0x200FFFFC
    MPU - Memory Region 1 End: 0x200FFFFF
    MPU - Enable or disable Memory Region 2: Disabled
    MPU - Memory Region 2 Start: 0x407FFFFC
    MPU - Memory Region 2 End: 0x400DFFFF
    MPU - Enable or disable Memory Region 3: Disabled
    MPU - Memory Region 3 Start: 0x400DFFFC
    MPU - Memory Region 3 End: 0x400DFFFF
    
  Synergy Common
    Main stack size (bytes): 0x1000
    Process stack size (bytes): 0
    Heap size (bytes) - A minimum of 4K (0x1000) is required if standard library functions are to be used.: 0x1000
    MCU Vcc (mV): 3300
    MCU Analog Power Supply AVCC0 (mV): 3300
    Parameter checking: Enabled
    Assert Failures: Return SSP_ERR_ASSERTION
    Error Log: No Error Log
    ID Code Mode: Unlocked (Ignore ID)
    ID Code (32 Hex Characters): FFFFFFFFFFFFFFFFFFFFFFFFFFFFFFFF
    
  Clocks
    XTAL 12000000Hz
    HOCO 48MHz
    Clock Src: HOCO
    ICLK Div /2
    PCLKB Div /2
    PCLKD Div /1
    FCLK Div /2
    Clock Src: HOCO
    SDADCCLK Div /12
    
  Pin Configurations
    TB_S1JA.pincfg -> g_bsp_pin_cfg
      ADREG 37 SDADC0_ADREG - - - - - - - 
      AVCC0 56 ANALOG0_AVCC0 - - - - - - - 
      AVCC1 39 ANALOG0_AVCC1 - - - - - - - 
      AVSS0 57 ANALOG0_AVSS0 - - - - - - - 
      AVSS1 40 ANALOG0_AVSS1 - - - - - - - 
      P000 63 - - - - Disabled - - "AGT1: AGTIO; CTSU0: TS16; GPT4: GTIOCB; ICU0: IRQ04; IIC0: SCL; KINT0: KRM0; SCI9: RXD; SCI9: SCL; SPI1: MISO" 
      P001 62 CTSU0_TS15 - Low None "Peripheral mode" - None "CTSU0: TS15; ICU0: IRQ00; RTC0: RTCOUT; SCI9: CTS; SPI1: RSPCK" 
      P002 61 - - - - Disabled - - "ADC0: AN07; DAC81: DA; OPAMP2: AMP+" 
      P003 60 ADC0_AN06 - - - "Analog mode" - None "ADC0: AN06; OPAMP2: AMP-" 
      P012 55 - - - - Disabled - - "ADC0: AN08; OPAMP2: AMPO" 
      P013 54 - - - - Disabled - - "ACMPHS0: IVCMP; ACMPHS0: IVREF; ADC0: AN05; DAC80: DA; GPT6: GTIOCB; OPAMP1: AMP+" 
      P014 53 - - - - Disabled - - "ACMPHS0: IVREF; ADC0: AN04; ANALOG0: VREFL; GPT6: GTIOCA; OPAMP1: AMP-" 
      P015 52 - - - - Disabled - - "ADC0: AN03; OPAMP1: AMPO" 
      P100 48 - - - - Disabled - - "ACMPHS0: IVCMP; ADC0: AN16; CTSU0: TS23; GPT5: GTIOCB; ICU0: IRQ04; SCI9: SDA; SCI9: TXD; SDADC0: ANSDP0" 
      P101 47 - - - - Disabled - - "ACMPHS0: IVREF; ADC0: AN17; CTSU0: TS22; GPT5: GTIOCA; ICU0: IRQ05; SCI9: RXD; SCI9: SCL; SDADC0: ANSDN0" 
      P102 46 - - - - Disabled - - "ADC0: AN18; CTSU0: TS21; GPT6: GTIOCB; SCI9: CTS; SDADC0: ANSDP1; SPI1: SSL0" 
      P103 45 - - - - Disabled - - "ADC0: AN19; CTSU0: TS20; GPT6: GTIOCA; SDADC0: ANSDN1; SPI1: RSPCK" 
      P104 44 - - - - Disabled - - "ADC0: AN20; CTSU0: TS19; ICU0: IRQ06; SDADC0: ANSDP2; SPI1: MISO" 
      P105 43 - - - - Disabled - - "ADC0: AN21; CTSU0: TS18; ICU0: IRQ07; SDADC0: ANSDN2; SPI1: MOSI" 
      P106 42 - - - - Disabled - - "ADC0: AN22; SDADC0: ANSDP3" 
      P107 41 - - - - Disabled - - "ADC0: AN23; SDADC0: ANSDN3" 
      P108 33 DEBUG0_SWDIO - Low - "Peripheral mode" - None "DEBUG0: SWDIO" 
      P109 64 - - - - Disabled - - "ACMP(0-1): VCOUT; ACMPLP0: CMPREF; ADC0: ADTRG; AGT0: AGTOA; CTSU0: TS17; GPT_POEG1: GTETRG; GPT1: GTIOCB; ICU0: IRQ03; IIC1: SCL; KINT0: KRM1; SCI0: SCK; SCI9: SDA; SCI9: TXD; SPI0: MISO" 
      P110 34 - - - - Disabled - - "ACMPLP1: CMPREF; ADC0: ADTRG; AGT0: AGTOB; CAN0: CTX; CGC0: CLKOUT; CTSU0: TSCAP; GPT_OPS0: GTOWLO; GPT2: GTIOCB; ICU0: IRQ02; IIC1: SDA; SCI0: SDA; SCI0: TXD; SCI9: RXD; SCI9: SCL; SPI0: RSPCK" 
      P111 35 - - - - Disabled - - "CTSU0: TS14; ICU0: IRQ06; IIC1: SCL; RTC0: RTCOUT; SPI0: RSPCK" 
      P112 36 GPIO nShutdown Low None "Output mode (Initial Low)" CMOS - "CGC0: CLKOUT; CTSU0: TSCAP; ICU0: IRQ07; IIC1: SDA; SPI0: SSL0" 
      P200 27 - - - - Disabled - - "ICU0: NMI" 
      P201 26 GPIO - - - "Input mode" - None "SYSTEM0: MD" 
      P204 24 - - - - Disabled - - "CTSU0: TS09; SCI0: RXD; SCI0: SCL; SCI9: SCK; SPI1: MOSI" 
      P205 23 GPIO - Low None "Output mode (Initial Low)" CMOS - "CTSU0: TS08; GPT_OPS0: GTOVLO; GPT3: GTIOCB; ICU0: IRQ00; IIC1: SDA; SCI0: SDA; SCI0: TXD; SCI1: CTS; SPI1: MISO" 
      P206 22 GPIO - - IRQ06 "Input mode" - None "AGT0: AGTIO; CTSU0: TS07; GPT_OPS0: GTOVUP; GPT3: GTIOCA; ICU0: IRQ06; IIC1: SCL; SCI0: CTS; SCI1: SDA; SCI1: TXD; SPI1: SSL0" 
      P212 10 - - - - Disabled - - "AGT0: AGTIO; CGC0: EXTAL; GPT_POEG1: GTETRG; GPT0: GTIOCB; ICU0: IRQ03; SCI1: SDA; SCI1: TXD" 
      P213 9 - - - - Disabled - - "AGT1: AGTEE; CGC0: XTAL; GPT_POEG0: GTETRG; GPT0: GTIOCA; ICU0: IRQ02; SCI1: RXD; SCI1: SCL" 
      P214 7 - - - - Disabled - - "CGC0: XCOUT" 
      P215 6 - - - - Disabled - - "CGC0: XCIN" 
      P300 32 DEBUG0_SWCLK - Low - "Peripheral mode" - None "DEBUG0: SWCLK" 
      P301 31 SCI0_RXD - Low None "Peripheral mode" CMOS None "AGT1: AGTOB; CTSU0: TS13; GPT_OPS0: GTOWUP; GPT2: GTIOCA; ICU0: IRQ05; IIC0: SDA; KINT0: KRM4; RTC0: RTCOUT; SCI0: RXD; SCI0: SCL; SCI9: CTS; SPI1: MOSI" 
      P302 30 SCI0_TXD - Low None "Peripheral mode" CMOS None "AGT1: AGTOA; CAC0: CACREF; CTSU0: TS12; GPT_OPS0: GTOVLO; GPT3: GTIOCB; ICU0: IRQ04; KINT0: KRM5; SCI0: SDA; SCI0: TXD; SCI1: RXD; SCI1: SCL; SPI1: RSPCK" 
      P303 29 GPIO - Low - "Output mode (Initial High)" - - "CAN0: CRX; CTSU0: TS11; GPT6: GTIOCB; KINT0: KRM6; SCI0: CTS; SCI1: SCK; SPI0: MOSI" 
      P304 28 GPIO - - - "Input mode" - None "CAN0: CTX; CTSU0: TS10; GPT6: GTIOCA; KINT0: KRM7; SCI0: SCK; SCI9: SDA; SCI9: TXD; SPI0: MISO" 
      P400 1 - - - - Disabled - - "ACMPLP0: CMPIN; AGT0: AGTEE; CTSU0: TS00; GPT_POEG0: GTETRG; GPT1: GTIOCA; ICU0: IRQ00; IIC1: SDA; KINT0: KRM2; RTC0: RTCOUT; SCI0: CTS; SCI1: RXD; SCI1: SCL; SPI0: MOSI" 
      P401 2 - - - - Disabled - - "ACMP(0-1): VCOUT; AGT1: AGTEE; CTSU0: TS01; GPT_OPS0: GTIU; GPT4: GTIOCA; ICU0: IRQ05; IIC0: SDA; KINT0: KRM3; SCI0: SCK; SCI9: SCK; SPI1: SSL1" 
      P402 3 - - - - Disabled - - "CTSU0: TS02; GPT_OPS0: GTIV; GPT0: GTIOCA; SCI9: CTS; SPI1: SSL2" 
      P403 4 - - - - Disabled - - "CTSU0: TS03; GPT_OPS0: GTIW; GPT0: GTIOCB; SCI1: SCK; SPI1: SSL3" 
      P407 16 USBFS0_VBUS - Low None "Peripheral mode" CMOS None "AGT0: AGTIO; CAC0: CACREF; CAN0: CTX; CTSU0: TSCAP; GPT_OPS0: GTOULO; GPT0: GTIOCB; ICU0: IRQ01; IIC0: SCL; SCI0: SDA; SCI0: TXD; SCI9: SDA; SCI9: TXD; SPI1: RSPCK; USB_FS0: VBUS; USB_FS0: VBUS" 
      P408 15 - - - - Disabled - - "ACMPLP1: CMPIN; AGT0: AGTO; CAN0: CRX; CTSU0: TS06; GPT_OPS0: GTOUUP; GPT0: GTIOCA; ICU0: IRQ01; IIC0: SDA; SCI0: RXD; SCI0: SCL; SCI1: SDA; SCI1: TXD; SPI0: SSL0" 
      P409 14 CTSU0_TSCAP - Low None "Peripheral mode" CMOS None "AGT1: AGTO; CAN0: CTX; CTSU0: TSCAP; GPT0: GTIOCA; ICU0: IRQ07; IIC0: SCL; SCI0: SCK; SCI1: CTS; SPI0: SSL1" 
      P410 13 - - - - Disabled - - "CTSU0: TS05; GPT5: GTIOCB; SCI0: CTS; SCI1: SDA; SCI1: TXD; SPI0: SSL2" 
      P411 12 - - - - Disabled - - "CTSU0: TS04; GPT5: GTIOCA; SCI0: SDA; SCI0: TXD; SCI1: RXD; SCI1: SCL; SPI0: SSL3" 
      P500 49 - - - - Disabled - - "ACMPHS0: IVCMP; ACMPHS0: IVREF; ADC0: AN00; CTSU0: TS24; DAC0: DA; GPT5: GTIOCA; ICU0: IRQ03; OPAMP0: AMP+; SCI0: RXD; SCI0: SCL" 
      P501 50 - - - - Disabled - - "ACMPHS0: IVREF; ADC0: AN01; CTSU0: TS25; GPT5: GTIOCB; ICU0: IRQ02; OPAMP0: AMP-; SCI0: SDA; SCI0: TXD" 
      P502 51 - - - - Disabled - - "ADC0: AN02; ICU0: IRQ01; OPAMP0: AMPO; SCI0: CTS" 
      P914 19 USBFS0_DP - - - "Peripheral mode" - - "USB_FS0: DP" 
      P915 18 USBFS0_DM - - - "Peripheral mode" - - "USB_FS0: DM" 
      RES# 25 SYSTEM0_RES - - - - - - - 
      SBIAS/VREFI 38 SDADC0_SBIAS - - - - - - - 
      VCC 11 SYSTEM0_VCC - - - - - - - 
      VCCUSB 20 USBFS0_VCC - - - - - - - 
      VCCUSBLDO 21 USBFS0_VCCLDO - - - - - - - 
      VCL 5 SYSTEM0_VCL - - - - - - - 
      VREFH - ANALOG0_VREFH - - - - - - - 
      VREFH0 59 ANALOG0_VREFH0 - - - - - - - 
      VREFL0 58 ANALOG0_VREFL0 - - - - - - - 
      VSS 8 SYSTEM0_VSS - - - - - - - 
      VSSUSB 17 USBFS0_VSS - - - - - - - 
      
  Module "CGC Driver on r_cgc"
    Parameter Checking: Default (BSP)
    Main Oscillator Wait Time: 2048 us (16384 cycles)
    Main Oscillator Clock Source: Crystal or Resonator
    Subclock Drive: Normal Mode
    Configure Subclock Drive On Reset: Enabled
    Low Voltage Mode: Disable
    
  Module "ELC Driver on r_elc"
    Parameter Checking: Default (BSP)
    
  Module "I/O Port Driver on r_ioport"
    Parameter Checking: Default (BSP)
    
  Module "FMI Driver on r_fmi"
    Parameter Checking: Default (BSP)
    SSP MCU Information Symbol Name: g_fmi_data
    Part Number Mask: 0xFE00
    
  Module "UART Driver on r_sci_uart"
    External RTS Operation: Disable
    Reception: Enable
    Transmission: Enable
    Parameter Checking: Default (BSP)
    
  Module "Transfer Driver on r_dtc"
    Parameter Checking: Default (BSP)
    Software Start: Disabled
    Linker section to keep DTC vector table: .ssp_dtc_vector_table
    
  Module "Timer Driver on r_gpt"
    Parameter Checking: Default (BSP)
    
  Module "Flash Driver on r_flash_lp"
    Parameter Checking: Default (BSP)
    Code Flash Programming Enable: Disabled
    
  HAL
    Instance "g_elc ELC Driver on r_elc"
      Name [Fixed]: g_elc
      
    Instance "g_cgc CGC Driver on r_cgc"
      Name [Fixed]: g_cgc
      
    Instance "g_ioport I/O Port Driver on r_ioport"
      Name [Fixed]: g_ioport
      
    Instance "g_fmi FMI Driver on r_fmi"
      Name: g_fmi
      
    Instance "g_uart0 UART Driver on r_sci_uart"
      Name: g_uart0
      Channel: 0
      Baud Rate: 115200
      Data Bits: 8bits
      Parity: None
      Stop Bits: 1bit
      CTS/RTS Selection: RTS (CTS is disabled)
      Name of UART callback function to be defined by user: user_uart_callback
      Name of UART callback function for the RTS external pin control to be defined by user: NULL
      Clock Source: Internal Clock
      Baudrate Clock Output from SCK pin: Disable
      Start bit detection: Falling Edge
      Noise Cancel: Disable
      Bit Rate Modulation Enable: Enable
      Receive FIFO Trigger Level: One
      Receive Interrupt Priority: Priority 2
      Transmit Interrupt Priority: Priority 2
      Transmit End Interrupt Priority: Priority 2
      Error Interrupt Priority: Disabled
      Baudrate Percent Error: 2.0
      UART Communication Mode: RS232
      UART RS485 Communication Mode: Half Duplex
      RS485 DE Port: 09
      RS485 DE Pin: 14
      
      Instance "g_transfer0 Transfer Driver on r_dtc SCI0 TXI"
        Name: g_transfer0
        Mode: Normal
        Transfer Size: 1 Byte
        Destination Address Mode: Fixed
        Source Address Mode: Incremented
        Repeat Area (Unused in Normal Mode): Source
        Interrupt Frequency: After all transfers have completed
        Destination Pointer: NULL
        Source Pointer: NULL
        Number of Transfers: 0
        Number of Blocks (Valid only in Block Mode): 0
        Activation Source (Must enable IRQ): SCI0 TXI
        Auto Enable: False
        Callback (Only valid with Software start): NULL
        ELC Software Event Interrupt Priority: Disabled
        
      Instance "g_transfer1 Transfer Driver on r_dtc SCI0 RXI"
        Name: g_transfer1
        Mode: Normal
        Transfer Size: 1 Byte
        Destination Address Mode: Incremented
        Source Address Mode: Fixed
        Repeat Area (Unused in Normal Mode): Destination
        Interrupt Frequency: After all transfers have completed
        Destination Pointer: NULL
        Source Pointer: NULL
        Number of Transfers: 0
        Number of Blocks (Valid only in Block Mode): 0
        Activation Source (Must enable IRQ): SCI0 RXI
        Auto Enable: False
        Callback (Only valid with Software start): NULL
        ELC Software Event Interrupt Priority: Disabled
        
    Instance "g_timer0 Timer Driver on r_gpt"
      Name: g_timer0
      Channel: 0
      Mode: Periodic
      Duty Cycle Range (only applicable in PWM mode): Shortest: 2 PCLK, Longest: (Period - 1) PCLK
      Period Value: 1
      Period Unit: Milliseconds
      Duty Cycle Value: 50
      Duty Cycle Unit: Unit Raw Counts
      Auto Start: True
      GTIOCA Output Enabled: False
      GTIOCA Stop Level: Pin Level Low
      GTIOCB Output Enabled: False
      GTIOCB Stop Level: Pin Level Low
      Callback: timer_1ms
      Overflow Interrupt Priority: Priority 3 (lowest - not valid if using ThreadX)
      
    Instance "g_flash0 Flash Driver on r_flash_lp"
      Name: g_flash0
      Data Flash Background Operation: Disabled
      Callback: NULL
      Flash Ready Interrupt Priority: Disabled
      
  Messaging
