-iwithprefixbefore/cores/rp2040/api/deprecated-avr-comp/
-iwithprefixbefore/include/pico_base/
-iwithprefixbefore/pico-sdk/lib/tinyusb/src/
-iwithprefixbefore/pico-sdk/src/boards/include
-iwithprefixbefore/pico-sdk/src/common/pico_base/include
-iwithprefixbefore/pico-sdk/src/common/pico_binary_info/include
-iwithprefixbefore/pico-sdk/src/common/pico_bit_ops/include
-iwithprefixbefore/pico-sdk/src/common/pico_divider/include
-iwithprefixbefore/pico-sdk/src/common/pico_stdlib/include
-iwithprefixbefore/pico-sdk/src/common/pico_sync/include
-iwithprefixbefore/pico-sdk/src/common/pico_time/include
-iwithprefixbefore/pico-sdk/src/common/pico_usb_reset_interface/include
-iwithprefixbefore/pico-sdk/src/common/pico_util/include
-iwithprefixbefore/pico-sdk/src/rp2040/hardware_regs/include
-iwithprefixbefore/pico-sdk/src/rp2040/hardware_structs/include
-iwithprefixbefore/pico-sdk/src/rp2_common/cmsis/include
-iwithprefixbefore/pico-sdk/src/rp2_common/cmsis/stub/CMSIS/Core/Include
-iwithprefixbefore/pico-sdk/src/rp2_common/cmsis/stub/CMSIS/Device/RaspberryPi/RP2040/Include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_adc/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_base/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_claim/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_clocks/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_divider/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_dma/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_exception/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_flash/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_gpio/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_i2c/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_interp/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_irq/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_rtc/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_pio/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_pll/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_pwm/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_resets/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_spi/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_sync/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_timer/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_uart/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_vreg/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_watchdog/include
-iwithprefixbefore/pico-sdk/src/rp2_common/hardware_xosc/include
-iwithprefixbefore/pico-sdk/src/rp2_common/pico_async_context/include
-iwithprefixbefore/pico-sdk/src/rp2_common/pico_bootrom/include
-iwithprefixbefore/pico-sdk/src/rp2_common/pico_btstack/include
-iwithprefixbefore/pico-sdk/src/rp2_common/pico_cyw43_arch/include
-iwithprefixbefore/pico-sdk/src/rp2_common/pico_cyw43_driver/include
-iwithprefixbefore/pico-sdk/src/rp2_common/pico_double/include
-iwithprefixbefore/pico-sdk/src/rp2_common/pico_float/include
-iwithprefixbefore/pico-sdk/src/rp2_common/pico_int64_ops/include
-iwithprefixbefore/pico-sdk/src/rp2_common/pico_lwip/include
-iwithprefixbefore/pico-sdk/src/rp2_common/pico_multicore/include
-iwithprefixbefore/pico-sdk/src/rp2_common/pico_platform/include
-iwithprefixbefore/pico-sdk/src/rp2_common/pico_printf/include
-iwithprefixbefore/pico-sdk/src/rp2_common/pico_runtime/include
-iwithprefixbefore/pico-sdk/src/rp2_common/pico_rand/include
-iwithprefixbefore/pico-sdk/src/rp2_common/pico_stdio/include
-iwithprefixbefore/pico-sdk/src/rp2_common/pico_stdio_uart/include
-iwithprefixbefore/pico-sdk/src/rp2_common/pico_unique_id/include
-iwithprefixbefore/pico-sdk/lib/cyw43-driver/src
-iwithprefixbefore/pico-sdk/lib/lwip/src/include
-iwithprefixbefore/pico-sdk/lib/btstack/src
-iwithprefixbefore/pico-sdk/lib/btstack/platform/embedded
